A Model A which has been restored is regularly driven and has *LIMITED* changes for driving comfort, convenience and safety. Vehicles in the touring class must be restored and be judged as defined in the *Guideline*s. Vehicles that enter this class may include any or all of the following non-original listed parts and shall receive no more than 50% of the points allotted for the individual component in its respective area.

Acceptable non-original items:

1   Overdrives (torque tube type)

2   Fan and hub (V belt driven)

3   Float-a-motor engine mounts

4   Carburetor (updraft only)

5   Electrical/Ignition System

6   Halogen or sealed beam headlights behind Model A lenses.

7   I2-volt conversion and/or an alternator

8   Steering box with original style column

9   Rubber valve stems

10   Manifold heaters

The following convenience and safety items will be allowed with no point deduction:

1 Turn signals

2 Seatbelts

3 Gauges

4 Fuses

5 Radios

6 2nd rear lamp and/or center brake light

7 Cast iron brake drums

# # # # # # #